**READ ME FIRST**

**This MAX 10 10M50 Development kit is supported with the Quartus II v15.0 Beta Software for MAX 10 (10M50). Follow these steps to install Quartus II and enable licensing:**

1. Create an account, validate your email, and download Quartus II Software from this cloud link:

<http://www.altera.com/10m50>

1. Send an email to [apgcs@altera.com](mailto:apgcs@altera.com) with your network interface card (NIC ID) and email address for a temporary fixed node license.

* To find your Windows NIC ID, type the following command at a command prompt:

**ipconfig /all**

In the output of the command, the NIC ID is the physical address without the dashes. If your PC has more than one network card, you can use the NIC ID of any network card connected to the computer that is turned on when the Quartus II software is in use.

* To find your Linux NIC ID, type the following command at a command prompt:

**/sbin/ifconfig eth0**

In the output of the command, the NIC ID is the ID to the right of **HWaddr**, without the colons.

1. When production license-free v15.0 becomes available at start of May 2015, update your Quartus II software from this site: <http://dl.altera.com/>